[Main]
NoEqSize =  doesn't match by the size
TestMode = TESTING MODE!!!
NoConfirm = Confirmation on the device screen wasn't selected!
RecFrBootP2 = After CWM Downloading in FlashTool, turn on phone only in the recovery mode! Press and retain volume-up with the Power button. The cable shall is connected to PC!
RecFrBootP = File /system/recovery-from-boot.p which restore factory recovery in case of phone switching on in a normal mode Is Found!
Att = ATTENTION!
NewVerExist =  There is a new version of the program
BadROM = ROM file is read from phone incorrectly!
FoundSU =  system/bin/su is found! Via the ROOT button it is possible to get root shell!
WrongHW =  Fake Hardware in kernel or firmware doesn't correspond to phone!
WrBlError = ERROR during write of the block
Timeout = Waiting time expired
Root4push = Confirm request on your device now! Select most bottom right option !
Created = It is created:
ADBexist = In system already available:
Root4 = temporary root shell will appear after two reboots!
Clean = cleaning
Contin = To continue?
CreateErr = can not create
Error = ERROR
File = file
Inaccessible = inaccessible
Install = install
InstallSkip = installation is skipped!
Installing = installing
Need = should be
NoFindF = file isn't found
NoMountRW = it was not remounted on ReadWrite!
NoOpenDir = I can not open archive
NoUtils = It was not possible to establish the utility in phone!
Not = not
NotSel = not selected
Pack = packing
Prepare = prepare
RecovNotSel = The file recovery.img isn't chosen,
ReplTo = it will be replaced on
SaveInFile = is write to the file:
SignErr = ERROR of a signature,
Signature = signature
UnknFmt = Unknown ROM structure, backup NOT possible!
WaitReboot = Expectation of reconnection of phone...
BadFstab = Recovery doesn't suit this phone!
WriteError = No free space or Write ERROR in file

[Back]
NoWrInRec = Write of created boot and recovery isn't allowed from the recovery mode. Use SP FlashTool.
UsePMT = Use it if SP FlashTool errors of 8038 or 4050 occurs 
PmtNotEql = Kernel Block Map to PMT mismatch!
NoKernlVer = I can't patch boot of this version yet
BootAlreadyPatch = Boot allready patched
SkipCre = skip creation new file
BadBP = Changed buid.prop is found
NoChangeBP = Changes in build_prop_replace.txt is not revealed
FreeSpaceError = ERROR, insufficiently free space
PhPcCopyError =  ERROR during copying file between phone and PC
PhFileError =  device create file ERROR
BlueHelios = Through CWM it is possible to get root on this phone! Look URLs
Del = we delete:
DelFiles = Removal of files from phone according to the list:
MTDReadErr = error of reading block
MTDSave = We keep blocks:
NoFile = We skip removal. The list for removal of files from phone isn't found:
NoSD = The SD card in phone isn't found!
PcDir = The preservation folder on the computer:
PhDir = In phone files will remain in the folder:
Pull = We keep folders contents copying on PC
RebootRecovery = Reboot in recovery
RecoveryOK = It is installed recovery from the file:
RootGet = it is received temporarily before reboot !
Skip2SD = The second partition SD of the card is found, saving of the section userdata will be passed!
TaskEnd = task is complete
TaskEndErr= task end with ERROR
Zip = We pack everything kept in archive:

[Yaffs]
Copy = Copy
Copied = it is copied
CopyEnd = copying is complete
CopyToDir = Check and copying of files in the folder:
Erasing = erasing
FTNotContinue = Preparation of files for FlashTool is impossible,
FileSize = too small size of the file;
MakedUpdate = update is created
NotCreate = IT IS NOT CREATED!
NotSign = The signature isn't found!
NotYaffs = The yaffs2 format isn't defined
Unpack = Unpacking of yaffs of the file
UnpackErr = when unpacking
UpdEnd = creation of updates for recovery is complete
UpdNoPossible = File creation update.zip it is impossible,
UserCancel = it is cancelled by the user.
YaffsOK = yaffs2 is unpacked an image in the folder:
dirToUpdate = Files for recovery will be created in the folder

[Text]
NvramTitle = IMEI and equipment calibrations are stored in NVRAM. BusyBox, Root shell or the CWM mode is necessary for full backup and restore NVRAM. TESTING MODE!!!
ImeiUnavail = Unavail in recovery mode. It possible only in case of normal switching on of the device
Su2 = Select application for SuperUser
Su1 = SuperSU is recommended for Android v4.2.1
Reboot1 = To reboot phone
Reboot2 = In usual or recovery mode
Reboot3 = Reboot
Reboot4 = in recovery
Reboot5 = Cancel
FreeROM = Free space
BlockInfo = Block devices information
BadMtd = The skatter wasn't possible to create the file. Unknown format
DisconnectDev = Communication with the phone is lost! Connect or reconnect a cable!
ImeiAhtung = ATTENTION! Function is intended only for restoration of the IMEI after dumping on factory settings, program failure or an insertion of the stranger of NVRAM!
NoConnectDev = The device isn't revealed. Connect or reconnect a cable!
Panel1Tab1 = Phone information
Panel1Tab2 = root, backup, recovery
TT_Imei = To enter the first 14 figures of IMEI
TmpUnpackErr = It is impossible to unpack temporary files!

[Buttons]
FromReadBack =    To process file ROM_ from FlashTool
TT_FromReadBack = To prepare files for FlashTool on the basis of the ROM file, received by Function ReadBack in FlashTool
 
recWrite = Install already prepared files
TT_recWrite = The chosen recovery and boot files for this phone are installed
recBootFile = To choose the boot.img file
TT_recBootFile = Are prepared patched boot and recovery on a basis recovery from similar phone
recBootPhone = To use boot from phone
TT_recBootPhone = Are prepared patched boot and recovery on a basis recovery from similar phone
BuildProp = Build.prop
TT_BuildProp = build.prop in phone according to the file build_prop_replace.txt changes
OnSD = Leave FlashTool files on SD card
TT_OnSD = Affects only files for FlashTool. Files for Recovery remain on SD always
BackCache = Backup userdata and cache
TT_BackCache = Contain personal data and settings. Are unessential to brick restoration.
Reboot = Reboot
TT_Reboot =  To reboot phone in usual or recovery mode
Return = Return
TT_Return = Exit in the previous window
1 = Execute task from Backup to Recovery
FilesToFT = To prepare blocks for FlashTool
TT_1 = To execute everything one after another one click
TT_FilesToFT = Check and preparation of files for flashing through FlashTool. In the new folder the files which have passed check are copied only.
TT_backup = To keep phone blocks on the computer and at existence on phone SD card.
TT_delete = The unnecessary applications which list is stored in the file files_for_delete.txt are removed
TT_imei = To replace one or two IMEI. Backup or restore NVRAM
TT_imeiNO = Exit in the previous window
TT_imeiOK = Replace
TT_info = To copy information on phone in a clipboard for the subsequent placement at a forum.
TT_recovery = recovery.img and patched boot.img is established or are prepared
TT_root = Get Temporary ROOT. Without it many functions are inaccessible and it is impossible to install SuperUser for permanent ROOT!
TT_scatter1 = To create scatter on the basis of already available firmware.info or pmt file.
TT_scatter2 = To create scatter for connected phone.
TT_su = For permanent root to install SuperUser and auxiliary programs
TT_term = the command Windows console in which it is possible to execute the ADB teams is started.
TT_unpack_yaffs = Unpacking of *.img of files in the yaffs2 format. Before unpacking md5 if the files.md5 file is available is checked.
TT_updates = Are checked md5, signatures and *_update.zip are created for sections: system, boot, recovery, uboot, logo, dsp_bl
backup = Backup
delete = Delete china
imei = IMEI/NVRAM
imeiNO = Cancelling
imeiOK = Replace IMEI
info = Info to clipboard
recovery = Recovery and Boot
root = ROOT
scatter1 = scatter from file
scatter2 = Create scatter file
su = SuperUser
term = ADB terminal
unpack_yaffs = To unpack yaffs2 the section
updates = To create updates for modified recovery
BlockInfo = Blocks Map
TT_BlockInfo = To show an arrangement of blocks in ROM

 

[MsgReq]
T_MakeCWM = If Not should choose CWM from similar phone.
MakeCWM = To make CWM recovery automatically?
T_RootAdbd = ATTENTION! Requests for confirmation on the device screen are possible!
RootAdbd =  To try to receive root shel through already established SU?      
T_noSD = ATTENTION! The SD card isn't found!
noSD = System and userdata won't backup! To continue? 
T_WrRecov = Recovery is created
WrRecov = Install created recovery to phone?
T_WrBoot = ATTENTION! There is a probability to damage the boot block!
WrBoot =  If phone isn't loaded, it is necessary to flash this file through FlashTool! Install patched boot to phone?
T_ZipBack = For reliable storage ...
ZipBack = Packing backup?
AdbLost = Loss of communication with the device! The programm will be closed!
Backup1 = For the subsequent restoration of phone it is necessary to keep phone sections ROM. It will take some minutes. To make it now?
DirExist = exists! If to continue, all data in the folder will be destroyed! To continue?
DirsExist = exist! If to continue, all data in folders will be destroyed! To continue?
ExistSU = Reinstall SuperUser, busybox, RootExplorer and MobileUncleTool?
FileExist = exists! If to continue, the file will be rewritten! To continue?
ImeInpErr = Few figures are entered. There should be not less than 14
ImeiEnd = Changes will come into force after reset.
NoAdb = It is impossible to start ADB!
NotCreateTmp = It is impossible to create the temporary folder!
RecovReboot = To reload phone in  recovery?
SuNotExist = Install SuperUser, busybox and RootExplorer?
T_AdbLost = CRITICAL ERROR!
T_Backup1 = It is necessary to keep ROM!
T_DirExist = Attention! The folder already exists!
T_DirsExist = Attention! Folders already exist!
T_ExistSU = Established SuperUser is found!
T_FileExist = Attention! File exists!
T_ImeInpErr = Error of input!
T_ImeiEnd = 
T_NoAdb = ERROR!
T_NotCreateTmp = ERROR!
T_RecovReboot = Recovery installed.
T_SuNotExist = Established SuperUser isn't found

[FSReq]
FileNotSelect = The file isn't chosen
FilesMd5 = Choose the files.md5 file in the folder with the backup...
RecovSel = Choose the recovery file for installation in phone. Cancellation - will not be established
ScatWr = Record scatter  file
SelectFile = Choose  file
BootSel = Choose the boot.img file from phone which you own ...
Recov2Sel = Choose the recovery file from similar phone ...
ModelName = Enter Phone name ...
RomSel = Choose ROM_ file which was received in the FlashTool, using a choice ReadBack ...